**Luxembourg (country code +352)**

Communication of 18.IV.2018:

The *Institut Luxembourgeois de Régulation (ILR),* Luxembourg*,* announces the following updates to national numbering plan in Luxembourg related to machine-to-machine (M2M) numbers.

a) Overview for M2M numbers:

The minimum number length (excluding the country code) is 12 digits.

The maximum number length (excluding the country code) is 12 digits.

b) Link to the national database (or any applicable list) with assigned ITU-T E.164 numbers within the national numbering plan:   
<https://web.ilr.lu/FR/Professionnels/Communications-electroniques/Numerotation/Numbering-Information-for-international-carriers/Pages/default.aspx>

c) Detail of numbering plan for M2M numbers:

| **NDC (national destination code) or leading digits of N(S)N (national (significant) number)** | **N(S)N number length** | | **Usage of E.164 number** | **Additional information** |
| --- | --- | --- | --- | --- |
| **Maximum length** | **Minimum length** |
| 6000 | 12 | 12 | M2M | MTX Connect S.à r.l. |
| 6001 | 12 | 12 | M2M | Join Experience S.A. |
| 6002 | 12 | 12 | M2M | Proximus S.A. |
| 6021 | 12 | 12 | M2M | POST Luxembourg |
| 6061 | 12 | 12 | M2M | Orange Communications Luxembourg S.A. |
| 6067 | 12 | 12 | M2M | Bouygues Telecom S.A. |

Contact:

Mr Jérôme Besch  
Institut Luxembourgeois de Régulation (ILR)  
17, rue du Fossé  
2922 Luxembourg  
Luxembourg  
Tel: +352 28 228 228  
Fax: +352 28 228 229  
E-mail: [numerotation@ilr.lu](mailto:numerotation@ilr.lu)  
URL: www.ilr.lu