**Moldova (country code +373)**

Communication of 6.IV.2016:

The *National Regulatory Agency for Electronic Communications and Information Technology*, Chisinau, announces that the following blocks of numbers were allocated to mobile network operators from the Republic of Moldova, during 2013-2015, and are still in use.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| *(1)* | *(2)* | | *(3)* | *(4)* |
| *NDC (National Destination Code) or leading digits of N(S)N (National (Significant) Number)* | *N(S)N number length* | | *Usage of ITU-T E.164 Number* | *Additional information* |
| *Maximum length* | *Minimum length* |
| 610, 611, 620, 621 | 8 | 8 | Mobile telephone service – JSC Orange Moldova | In use |
| 760, 767 | 8 | 8 | Mobile telephone service – JSC Moldcell | In use |
| 677 | 8 | 8 | Mobile telephone service – JSC Moldtelecom Unite | In use |

Contact:

National Regulatory Agency for Electronic Communications   
and Information Technology (ANRCETI)  
134, Stefan cel Mare Bv.  
CHISINAU 2012  
Moldova  
Tel: +373 2225 1317  
Fax: +373 2222 2885  
E-mail: office@anrceti.md  
URL: www.anrceti.md

The *National* *Regulatory Agency for Electronic Communications and Information Technology*, Chisinau, is announcing about the modifications made to the National Numbering Plan of the Republic of Moldova.

As of 1 April 2012, Moldova implemented the “closed” type of dialling geographical numbers on its territory.

Geographic numbers in the country are dialled as follows: prefix”0” and the national significant number (N(S)N).

The use of prefix “0” is temporary.

The dialling of telephone numbers from outside of Moldova has not been modified: they are dialled as follows: country code of the Republic of Moldova (+373) and the national significant number (N(S)N).

The maximum length of a national significant number is eight (8) digits.

The table below provides information on the most recent modifications of the National Numbering Plan of the Republic of Moldova.

| *NDC (National Destination Code) or leading digits of N(S)N (National (Significant) Number)* | *N(S)N Number length* | | *Usage of E.164 Number* | *Additional information* |
| --- | --- | --- | --- | --- |
| *Minimum* | *Maximum* |
| 0 | 1 | 1 | National prefix |  |
| 00 | 2 | 2 | International prefix |  |
| 1010 – 1099 | 4 | 4 | Carrier access codes |  |
| 112 | 3 | 3 | Short number for calling the emergency service |  |
| 113 - 115 |  |  |  | Reserved |
| 116 | 6 | 6 | Harmonized numbers for harmonized services of social value |  |
| 117 |  |  |  | Reserved |
| 118 | 4 | 5 | Short numbers for information inquiry | In use |
| 119 |  |  |  | Reserved |
| 12 - 13 |  |  |  | Reserved |
| 14 | 5 | 5 | Short numbers for a services | Services of general interest |
| 15 |  |  |  | Reserved |
| 1600 – 1639 | 4 | 4 | Access codes | In use |
| 17 | 4 | 4 | Routing numbers |  |
| 18 |  |  |  | Reserved |
| 19 | 4 | 4 | Access codes | Access to data transport services |
| 210 – 219, 22, 230 - 299 | 8 | 8 | Geographic numbers |  |
| 30, 38 | 8 | 8 | Nomadic numbers | In use |
| 31- 37, 39 | 8 | 8 | Geographic numbers |  |
| 533, 552, 555, 557 | 8 | 8 | Geographic numbers |  |
| 60 – 69 | 8 | 8 | Mobile telephone numbers |  |
| 71 | 8 | 8 | Mobile telephone numbers for MVNO |  |
| 760, 767 | 8 | 8 | Mobile telephone numbers |  |
| 78, 79 | 8 | 8 | Mobile telephone numbers |  |
| 800 | 8 | 8 | Free phone numbers | In use |
| 803 | 8 | 8 | Universal access numbers |  |
| 808 | 8 | 8 | Shared cost numbers |  |
| 814 | 8 | 8 | Numbers for services | Transport services |
| 821 | 8 | 8 | Numbers for services | Internet access service |
| 900 | 8 | 8 | Premium rate numbers | In use |
| 905 | 8 | 8 | Premium rate numbers | In use |
| 906 | 8 | 8 | Premium rate numbers | In use |

Mobile numbers

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| *NDC (National Destination Code) or leading digits of  N(S)N (National (Significant) Number)* | *N(S)N number length* | | *Usage of E.164 Number* | *Additional information* |
| *Maximum length* | *Minimum length* |
| 60, 68, 69 | 8 digits | 8 digits | Mobile telephone service (GSM) – Orange Moldova | In use |
| 610, 611, 620, 621 | 8 digits | 8 digits | Mobile telephone service – JSC Orange Moldova | In use |
| 671 – 674 | 8 digits | 8 digits | Mobile telephone service (CDMA) – Moldtelecom S.A Unite | In use |
| 675, 676 | 8 digits | 8 digits | Mobile telephone service (GSM) – JSC Moldtelecom Unite | In use |
| 677 | 8 digits | 8 digits | Mobile telephone service – JSC Moldtelecom Unite | In use |
| 760 | 8 digits | 8 digits | Mobile telephone service – JSC Moldcell | In use |
| 767 | 8 digits | 8 digits | Mobile telephone service (GSM) – JSC Moldcell | In use |
| 780 – 788, 79 | 8 digits | 8 digits | Mobile telephone service (GSM) – Moldcell | In use |

Contact:

National Regulatory Agency for Electronic Communications   
and Information Technology (ANRCETI)  
134, Stefan cel Mare Bv.  
CHISINAU 2012  
Moldova  
Tel: +373 2225 1317  
Fax: +373 2222 2885  
E-mail: office@anrceti.md  
URL: www.anrceti.md